Receipt
Printer
EPSON
TM-U200 series
Printer
The standard POS printer model is more
powerful than ever.
The TM-U200 family offers a receipt printer that is
compact, reliable, and comes in two different
colors to blend with any atmosphere. It also boasts
a multitude of user-friendly features including an
Auto Status Back (ASB), journal take-up, and
receipt cutter. The TM-U200 series is in wide use as
the POS standard printer for the general retail,
restaurant kitchen and hospitality markets.
Compact, Fast and
Reliable
The TM-U200 series has been
equipped with numerous features
that maximize ease-of-use,
including drop-in roll paper
loading, an Auto Status Back
function, an autocutter (Type A
and B), and a journal take-up
device (Type A). Not only do these
easy-to-use features save time, they
also make employee training fast
and efficient.
Flexible, and with a
Multitude of Applications
Two-color printing, in black and
red. Freely adjustable paper-loading
pitch. A nearly universal ESC/
POS-compliant control code that
enables customization of receipts by
users. EPSON OCX driver support.
The flexibility of the TM-U200
series makes it easy to develop
original POS application software
without spending a lot of time and
money. The auto status back
function automatically transmits
changes in the printer status.
Easy to Exchange the
Roll Paper
The new Type A model is equipped
with a take-up device. It has also
been developed to enable easy
removal of journal paper. These
improvements make the task of
exchanging paper even faster and
easier.
Smart technology. Smart business. EPSON
Epson America, Inc. • 3840 Kilroy Airport Way • Long Beach, CA 90806 • Product Purchase Referral Line: (562) 290-5304
© 2000 Epson America, Inc. EPSON and ESC/POS are registered trademarks of Seiko Epson Corporation.
Connect-It is a trademark of Epson America, Inc. EPSON is a member of the OPOS committee.
Receipt
Printer
EPSON TM-U200 series Printer
Inch values are approximate.
cpi: characters per 25.4 mm (characters per inch)
lps: lines per second
* To find out more about our line of Connect-It Interfaces talk to your EPSON Sales Representative.
Specifications are subject to change without notice. Conforms to OLE POS specifications.
TM-U200 Specifications
Print Method 9-pin, serial impact dot matrix
Print Font 7 × 9 / 9 × 9
Column capacity 40 or 42 columns / 33 or 35 columns
Character size
1.24 × 3.1 mm (W × H) / 1.56 × 3.1 mm (W × H)
{0.049 × 0.122" / 0.061 × 0.122"}
Character set
95 Alphanumeric, 32 International, 128 × 8 Graphics
Traditional / Simple Chinese, Thai, Japanese (Type A)
Print Speed Approx. 3.5 lps (40 columns, 16 cpi) / Approx. 6.4 lps (16 columns, 16 cpi)
Data Buffer 1 KB or 40 bytes
Interfaces RS-232C / Bi-directional parallel / RS-485 / Connect-It*
Paper 76 ± 0.5 × diameter 83 mm {2.99 ± 0.02 × diameter 3.27"} (roll)
Paper Thickness 0.06 to 0.085 mm {0.0024 to 0.0033"}
Copy Capability One original and two copies for Type D; one original and one copy for other models
Inked Ribbon ERC-38 (purple, black, black / red)
Ribbon Life
Purple: 4,000,000 characters, Black: 3,000,000 characters,
B/R: 1,500,000 characters (black) 750,000 characters (red)
Power Supply AC adapter (included), PS-170 (option)
Power Consumption Approx. 43 W average
D.K.D. Function 2 drivers
Reliability
MTBF 180,000 hours
MCBF 18,000,000 lines
Overall Dimensions
Type A: 160 × 295 × 160 mm (W × D × H) {6.30 × 11.61 × 6.30"}
Type B: 160 × 248 × 150 mm (W × D × H) {6.30 × 9.76 × 5.91"}
Type D: 160 × 248 × 133 mm (W × D × H) {6.30 × 9.76 × 5.24"}
Mass
Type A and B: Approx. 2.5 kg {5.51 lb}
Type D: Approx. 2.2 kg {4.85 lb}
EMI Standards VCCI class A, FCC class A, CE marking, AS/NZS 3548
Safety Standards UL, CSA, EN60950
EPSON