•	Magnetic Card Reader Failures  --  Local Terminal
 
      		**** Cancel to Return ****

POS Magnetic Reader Common Problems and Cause:

Card does NOT read:

Card reader is dirty (contaminated) and needs cleaning.
Card magnetic strip damaged or worn.
Card magnetic strip incorrect format (incompatibility).
Card type not accepted by system.
Read not allowed based on server CLASSIFICATION.
Read not allowed at current prompt in system.
Card reader not connected to POS.
Card reader cable damaged.

Information Missing in read:

Track 2 only reader.
Magnetic strip damage.
Incorrect Manufactures software drivers installed.

Integrated Reader problems:

Incorrect Manufactures software drivers installed.
Internal cables disconnected.
Console prompt setup variables incorrect.